IFC building model
Schema: "IFC4"
Description: "no view"
File name: "3D-Modell 100993.73.ifc"
Time stamp: "2023-10-16T09:09:24"
Author: "Tridici Gioele"
Organization: "No Organization"
Preprocessor: "EDMsix Version 2.0.209.92 Dec 12 2020"
Originating system: "Allplan 2023.1 06.07.2023 - 11:36:50"
Application: "Allplan" version "2023.1" identifier "Allplan" by Organization "No Organization"

People and organizations
  Person "Tridici" "Gioele" of Organization "No Organization"
  Owner history of Person "Tridici" "Gioele" of Organization "No Organization" | application "Allplan" version "2023.1" identifier "Allplan" by Organization "No Organization" | change NOTDEFINED | created 1697440163 (2023-10-16T07:09:23Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  PLANEANGLEUNIT: DEGREE (conversion based)
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived

Spatial structure
IFCPROJECT "D Leitungsbau"
  IFCSITE "D0001 Kabelkanäle mit Deckel" | latitude 48° 8′ 10.32″ | longitude 11° 41′ 19.32″
    IFCBUILDING "Deckel" | COMPLEX
      IFCBUILDINGSTOREY "Art. Nr. 100993.73 Typ 23 Deckel bewehrt" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | names: "" | property sets: AllplanAttributes

Property sets
  AllplanAttributes | properties | on 1 object (1 IFCPROJECT)
    Architect = "Architekt Name" (IFCTEXT)
    Architect, ZIP code/city = "Architekt PLZ Ort" (IFCTEXT)
    Architect, street = "Architekt Strasse" (IFCTEXT)
    Building contractor = "Bauunternehmer Name" (IFCTEXT)
    Building contractor, ZIP code/city = "Bauunternehmer PLZ Ort" (IFCTEXT)
    Building contractor, street = "Bauunternehmer Strasse" (IFCTEXT)
    Client = "Bauherr Name" (IFCTEXT)
    Client, ZIP code/city = "Bauherr PLZ Ort" (IFCTEXT)
    Client, street = "Bauherr Strasse" (IFCTEXT)
    Construction site = "PLZ und Ort" (IFCTEXT)
    Project description = "Projektbeschreibung" (IFCTEXT)
    Project number = "D" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Allright_Comp_ID = "0071AdE0000000001" (IFCTEXT)
    CBB_Artikelnummer = "119804.71" (IFCTEXT)
    CBB_Ausführung = "Sofortentschalt" (IFCTEXT)
    CBB_Brauen = "Werden mechanisch entfernt" (IFCTEXT)
    CBB_Breite B = 350 (IFCINTEGER)
    CBB_Dokument = "D0001-HW71:2020 Kabelkanaldeckel" (IFCTEXT)
    CBB_Druckfestigkeitsklasse C = "C40/50" (IFCTEXT)
    CBB_Expositionsklasse EK = "XC4 / XD1 / XF3" (IFCTEXT)
    CBB_Gewicht G = "20" (IFCTEXT)
    CBB_Herstellwerk = "HW71" (IFCTEXT)
    CBB_Höhe H = 50 (IFCINTEGER)
    CBB_Höhe h1 = 45 (IFCINTEGER)
    CBB_Kantenbeschaffenheit = "obere Kanten gefast 3/3 mm" (IFCTEXT)
    CBB_Klasse des Chloridgehaltes = "CI 0.1" (IFCTEXT)
    CBB_Korndurchmesser Dmax = 8 (IFCINTEGER)
    CBB_Länge L = 500 (IFCINTEGER)
    CBB_Material = "Stahlbeton" (IFCTEXT)
    CBB_Maximale Porenanzahl pro Fläche = "5" (IFCTEXT)
    CBB_Maximale Porentiefe tp = 5 (IFCINTEGER)
    CBB_Maximaler Porendurchmesser dp = 10 (IFCINTEGER)
    CBB_Name = "Kabelkanaldeckel Typ 23 bewehrt" (IFCTEXT)
    CBB_Rissbreite = "Zulässig bis 0.15 mm" (IFCTEXT)
    CBB_Rubrik = "D0001" (IFCTEXT)
    CBB_Wasseraufnahme = "Die Wasseraufnahme des Betons darf 6% seiner Masse nicht überschreiten." (IFCTEXT)
    Calculation mode = "m³" (IFCTEXT)
    Object_name = "Quader" (IFCTEXT)