IFC building model
Schema: "IFC4"
Description: "no view"
File name: "3D-Modell 100102.16.ifc"
Time stamp: "2025-07-15T10:36:16"
Author: "Fankhauser Tim"
Organization: "No Organization"
Preprocessor: "EDMsix Version 2.0.209.92 Dec 12 2020"
Originating system: "Allplan 2023.1 06.02.2025 - 14:42:46"
Application: "Allplan" version "2023.1" identifier "Allplan" by Organization "No Organization"

People and organizations
  Person "Fankhauser" "Tim" of Organization "No Organization"
  Owner history of Person "Fankhauser" "Tim" of Organization "No Organization" | application "Allplan" version "2023.1" identifier "Allplan" by Organization "No Organization" | change NOTDEFINED | created 1752568571 (2025-07-15T08:36:11Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  PLANEANGLEUNIT: DEGREE (conversion based)
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived

Spatial structure
IFCPROJECT "D Leitungsbau"
  IFCSITE "D1110 ASTRA Kabelschächte" | latitude 48° 8′ 10.32″ | longitude 11° 41′ 19.32″
    IFCBUILDING "Kabelschächte S mit Fundament"
      IFCBUILDINGSTOREY "Art. Nr. 100102.16 S1 600 / 1000 / 65" | elevation 0.
        contains 11 elements
          11 x IFCBUILDINGELEMENTPROXY | names: "", "SA 5.0-50 - C.99.570481", "LB 200-200 - C.99.530213.4" | material: "Beton Vorfabriziert" | property sets: AllplanAttributes, Pset_BuildingElementProxyCommon

Property sets
  AllplanAttributes | properties | on 1 object (1 IFCPROJECT)
    Projektnummer = "D" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abrechnungsart = "m³" (IFCTEXT)
    Allright_Bauteil_ID = "1626ErE0000178728" (IFCTEXT)
    Objektname = "Erweitertes Element" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abrechnungsart = "m³" (IFCTEXT)
    Allright_Bauteil_ID = "1626ErE0000178729" (IFCTEXT)
    Objektname = "Erweitertes Element" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abrechnungsart = "m³" (IFCTEXT)
    Allright_Bauteil_ID = "1626ErE0000178730" (IFCTEXT)
    Objektname = "Erweitertes Element" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abrechnungsart = "m²" (IFCTEXT)
    Allright_Bauteil_ID = "1626ErE0000178731" (IFCTEXT)
    Gewerk = "Betonarbeiten" (IFCTEXT)
    Material = "Beton Vorfabriziert" (IFCTEXT)
    Objektname = "Erweitertes Element" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abrechnungsart = "St" (IFCTEXT)
    Allright_Bauteil_ID = "1626PEb0000178735" (IFCTEXT)
    Antwort 1 = "SA" (IFCTEXT)
    Antwort 2 = "5.0" (IFCTEXT)
    Antwort 3 = "50" (IFCTEXT)
    Antwort 4 = "verz." (IFCTEXT)
    Antwort 5 = "Rd12" (IFCTEXT)
    Bezeichnung = "SA 5.0-50 - C.99.570481" (IFCTEXT)
    Frage 1 = "Typ" (IFCTEXT)
    Frage 2 = "Last" (IFCTEXT)
    Frage 3 = "Länge" (IFCTEXT)
    Frage 4 = "Material" (IFCTEXT)
    Frage 5 = "Gewinde" (IFCTEXT)
    Index Maßkette = 0 (IFCINTEGER)
    OK = 0. (IFCLENGTHMEASURE) [METRE]
    Objektname = "Punkt-Einbauteil" (IFCTEXT)
    UK = 0. (IFCLENGTHMEASURE) [METRE]
    V6 = 0. (IFCLENGTHMEASURE) [METRE]
    V7 = 0. (IFCLENGTHMEASURE) [METRE]
    V8 = 0. (IFCLENGTHMEASURE) [METRE]
    V9 = 0. (IFCREAL)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abrechnungsart = "m²" (IFCTEXT)
    Allright_Bauteil_ID = "1626ErE0000178743" (IFCTEXT)
    Gewerk = "Betonarbeiten" (IFCTEXT)
    Material = "Beton Vorfabriziert" (IFCTEXT)
    Objektname = "Erweitertes Element" (IFCTEXT)
  AllplanAttributes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Abrechnungsart = "m²" (IFCTEXT)
    Allright_Bauteil_ID = "1626ErE0000178740" (IFCTEXT)
    Gewerk = "Betonarbeiten" (IFCTEXT)
    Material = "Beton Vorfabriziert" (IFCTEXT)
    Objektname = "Erweitertes Element" (IFCTEXT)
  AllplanAttributes: 4 more contents on 4 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    LoadBearing = TRUE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)